**The CATALOGUE**

**Chart papers in rolls or z-folded for medical recording devices**

**Manufactured by CJSC «Factory of Chart Paper»**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| № | Registry number | **Design style** |  | Dimensions | Core size, mm | The presence of diagram grid | Winding of the diagram grid and thermal layer on the core | The presence of the mark | The presence of the perforation | Material | Basic weight gr/ sq.m | Compatible equipment | Pcs in the box. | Sq.m in 1 roll or in 1 pack |  |
| 1 | 4017 | **8** | roll | 44х30 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** | 90 | 1,32 |  |
| 2 | 4018 | **2** | roll | 50х30 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** Hellige etc. | 119 | 1,50 |  |
| 3 | 4018/1 | **4** | roll | 50х30 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** KENZ etc. | 119 | 1,50 |  |
| 4 | 4018/2 | **8** | roll | 50х30 | 18 | No | outward | No mark |  | Thermal paper | 55 | **ECG** | 119 | 1,50 |  |
| 5 | 4018/3 | **6** | roll | 50х30 | 18 | No | inward | No mark |  | Thermal paper | 55 | **ECG** | 119 | 1,50 |  |
| 6 | 4018/4 | **2** | roll | 50х25 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** | 84 | 1,25 |  |
| 7 | 4018/5 | **8** | roll | 50х45 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** |  | 2,25 |  |
| 8 | 4018/6 | **8** | roll | 50х28 | 18 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** | 98 | 1,4 |  |
| 9 | 4019 | **3** | roll | 50х25 | 18 | Yes | outward | Yes |  | Thermal paper | 55 | **ECG** Elektronika Trentina, Dixion ECG 1001 and etc. | 84 | 1,25 |  |
| 10 | 4020 | **3** | roll | 50х30 | 18 | Yes | outward | Yes |  | Thermal paper | 55 | **ECG** Cardioline ETA 150 and etc. | 75 | 1,50 |  |
| 11 | 4023 | **2** | roll | 50х50 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** 1-canal. , EC 1Т, «Malysh», Axion, Salut and etc | 40 | 2,50 |  |
| 12 | 4023/1 | **8** | roll | 50х50 | 18 | No | outward | No mark |  | Thermal paper | 55 | **ECG** | 40 | 2,50 |  |
| 13 | 4023/2 | **4** | roll | 50х50 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG Valenta and etc.** | 40 | 2,50 |  |
| 14 | 4023/3 | **6** | roll | 50х5018 |  | No | inward | No mark |  | Thermal paper | 55 | **Laboratory equipment** | 40 | 2,50 |  |
| 15 | 4024 | **8** | roll | 57х20 | 12 | No | outward | No mark |  | Thermal paper | 55 | **- Laboratory equipment (biochemical analyzer)** AVО, Bosh, Advia-60,HP,Epson, Multiscan,Biochem FP-900,  - autorefractometer GR-2100,  - **impedance meter** AZ-26 and etc. | 100 | 1,14 |  |
| 16 | 4024/1 | **8** | roll | 55х30 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** Mindrey ВА-88А and etc. | 68 | 1,65 |  |
| 17 | 4024/2 | **8** | roll | 57х30 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment (biochemical analyzer)**, Biosys Guardian BPM 700/730, **coagulometer** Sysmex and etc. | 72 | 1,71 |  |
| 18 | 4024/3 | **8** | roll | 57х25 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment breathalyzer** Lion SD-400P and etc | 72 | 1,43 |  |
| 19 | 4024/4 | **8** | roll | 57х23 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment, biochemical analyzer, etc.** | 84 | 1,31 |  |
| 20 | 4024/5 | **8** | roll | 57х10 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment, biochemical analyzer, etc.** | 175 | 0,57 |  |
| 21 | 4024/6 | **8** | roll | 57х50 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment, biochemical analyzer, etc.** | 40 | 2,85 |  |
| 22 | 4024/7 | **8** | roll | 57х7 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment, etc.** | 200 | 0,40 |  |
| 23 | 4024/8 | **8** | roll | 58х15 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment, etc.** | 128 | 0,87 |  |
| 24 | 4024/9 | **8** | roll | 57х15 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment, etc.** | 120 | 0,86 |  |
| 25 | 4024/10 | **8** | roll | 57х40 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment, etc.** | 40 | 2,28 |  |
| 26 | 4024/11 | **8** | roll | 57х32 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment, etc.** | 70 | 1,82 |  |
| 27 | 4024/12 | **8** | roll | 57х47 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment, etc.** |  | 2,68 |  |
| 28 | 4025 | **4** | roll | 57х23 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** Heartmirror, EC 1Т-07, «Aksion» Ucard 60, EC ZТ-01-R-D, Heart Screen 60G, Alton-103 , etc | 84 | 1,31 |  |
| 29 | 4025 /0 | **2** | roll | 57х23 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | **Defibrillator** EC 1Т-07 «Aksion» , etc. | 84 | 1,31 |  |
| 30 | 4025/1 | **2** | roll | 57х30 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG, Laboratory equipment, etc**. | 72 | 1,71 |  |
| 31 | 4025/2 | **2** | roll | 58х30 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** Heartmirror, etc. | 72 | 1,74 |  |
| 32 | 4025/3 | **4** | roll | 58х23 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** | 84 | 1,33 |  |
| 33 | 4025/4 | **4** | roll | 57х18 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** Alton-103 , etc. | 96 | 1,03 |  |
| 34 | 4025/5 | **4** | roll | 57х50 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** Alton-103 , etc | 40 | 2,85 |  |
| 35 | 4025/6 | **4** | roll | 57х25 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** Alton-103, etc. | 72 | 1,43 |  |
| 35 | 4025/7 | **4** | roll | 58х25 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** BTL-08 S-lines, etc. | 72 | 1,45 |  |
| 37 | 4025/8 | **2** | roll | 57х25 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** | 72 | 1,43 |  |
| 38 | 4025/9 | **4** | roll | 57х20 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** | 100 | 1,14 |  |
| 39 | 4025/10 | **4** | roll | 57х30 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** | 72 | 1,71 |  |
| 40 | 4025/11 | **4** | roll | 57х15 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG Alton, etc**. | 100 | 0,85 |  |
| 41 | 4025/12 | **2** | roll | 57х15 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** ECZТ-01-R-D , etc. | 100 | 0,85 |  |
| 42 | 4025/13 | **8** | roll | 58х30 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** |  | 1,74 |  |
| 43 | 4025/14 | **8** | roll | 57х6 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Breathalyzer** | 220 | 0,34 |  |
| 44 | 4025/15 | **8** | roll | 58х27 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** |  | 1,57 |  |
| 45 | 4026 | **8** | roll | 60х75 | 13 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment biochemical analyzer** Uitarograph , etc. | 30 | 4,50 |  |
| 46 | 4026/1 | **4** | roll | 60х30 | 16 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** Cardioline Delta 1 Plus , etc. | 68 | 1,80 |  |
| 47 | 4026/2 | **8** | roll | 60х30 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** Uitarograph , etc. | 72 | 1,80 |  |
| 48 | 4027 | **2** | roll | 63х30 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** Burdic, Cardisuny, Fucuda ,FX-2111, Hellige, Kenz, Nihon Kohden, ECG 9803, Medinova, Biocare ECG-300G, FX-7102 , etc. | 63 | 1,89 |  |
| 49 | 4027/1 | **10** | z-fold pack | 63х75х400 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Fucuda FX-7102, ,Nihon Kohden, Siemens **Cardiostat** 11 , etc. | 60 | 1,89 |  |
| 50 | 4027/2 | **2** | roll | 63х30 | 16 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** Hellige, Kenz, Nihon Kohden, Fukuda FX 2111 , etc. | 63 | 1,89 |  |
| 51 | 4027/3 | **4** | roll | 63х30 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** | 63 | 1,89 |  |
| 52 | 4027/4 | **2** | roll | 63х20 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** Fukuda , etc. | 77 | 1,26 |  |
| 53 | 4028 | **10** | z-fold pack | 70х100х200 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Schiller AT-3, **defibrillator** Corpuls 08/16 , etc. | 80 | 1,40 |  |
| 54 | 4029 | **8** | roll | 80х30 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment biochemical analyzer** BHA AYL, BHAAYO,  **spiroanalyzer** etc. | 51 | 2,40 |  |
| 55 | 4029/1 | **6** | roll | 80х30 | 12 | No | inward | No mark |  | Thermal paper | 55 | **Laboratory equipment biochemical analyzer** BHА AYL, BHА AYO,  spiroanalyzer, etc. | 51 | 2,40 |  |
| 56 | 4029/2 | **10** | z-fold pack | 80х90х280 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** MAC-400 , MAC-600 , etc. | 39 | 2,02 |  |
| 57 | 4029/3 | **8** | roll | 80х20 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment biochemical analyzer** BHА AYL, BHА AYO,,  **spiroanalyzer**, etc. | 73 | 1,60 |  |
| 58 | 4029/4 | **8** | roll | 80х74 | 18 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** |  | 5,92 |  |
| 59 | 4030 | **4** | roll | 80х30 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** Heart Scren 80G, Heart Mirror, Innomed, Dixion ЕСG, Kenz Cardico 306 , etc. | 51 | 2,40 |  |
| 60 | 4030/1 | **4** | roll | 80х30 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** 3rd can. Ucard, ECG Medinov, Heart Screen , etc. | 51 | 2,40 |  |
| 61 | 4030/2 | **4** | roll | 80х23 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** | 63 | 1,84 |  |
| 62 | 4030/3 | **4** | roll | 80х20 | 16 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** MAC-600 , etc. | 63 | 1,60 |  |
| 63 | 4030/4 | **2** | roll | 80х23 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | ECG | 63 | 1,84 |  |
| 64 | 4030/5 | **2** | roll | 80х30 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | ECG | 51 | 2,40 |  |
| 65 | 4030/6 | **4** | roll | 80х25 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | ECG | 54 | 2,00 |  |
| 66 | 4030/7 | **2** | roll | 80х30 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | ECG | 51 | 2,40 |  |
| 67 | 4030/8 | **2** | roll | 80х20 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | ECG | 73 | 1,60 |  |
| 68 | 4030/9 | **4** | roll | 80х20 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | ECG | 73 | 1,6 |  |
| 69 | 4030/10 | **4** | roll | 80х25 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** | 68 | 2,0 |  |
| 70 | 4030/11 | **8** | roll | 80х60 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** | 24 | 4,8 |  |
| 71 | 4031 | **2** | roll | 90х50 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** 2 canals, EC 2Т, MAC-500 , etc. | 36 | 4,50 |  |
| 72 | 4031/1 | **2** | roll | 90х30 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | ECG | 48 | 2,7 |  |
| 73 | 4031/2 | **4** | roll | 90х50 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | ECG | 36 | 4,5 |  |
| 74 | 4031/3 | **5** | roll | 90х30 | 18 | No | inward | Yes |  | Thermal paper | 55 | ECG | 48 | 2,7 |  |
| 75 | 4031/4 | **7** | roll | 90х30 | 18 | No | outward | Yes |  | Thermal paper | 55 | ECG | 48 | 2,7 |  |
| 76 | 4032 | **10** | z-fold pack | 90х70х400 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Biomedica P 80 , etc. | 45 | 2,52 |  |
| 77 | 4033 | **10** | z-fold pack | 90х90х400 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Schiller AT-1 ,Spirovit SP 1, etc. | 36 | 3,24 |  |
| 78 | 4033/1 | **10** | z-fold pack | 90х90х270 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Schiller AT-4 , AT-104, **defibrillator** Zoll M-series , etc. | 50 | 2,19 |  |
| 79 | 4033/2 | **10** | z-fold pack | 90х90х200 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Schiller AT-4 , AT-104, **defibrillator** Zoll M-series , etc. | 72 | 1,62 |  |
| 80 | 4034 | **9** | z-fold pack | 100х100х150 |  | Yes |  | No mark |  | Thermal paper | 55 | **Fetal monitor FM** Wakelingmedical AFM 210 , etc. | 90 | 1,50 |  |
| 81 | 4035 | **10** | z-fold pack | 107х140х200 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Burdick Eclipse 400, 4/400 , etc. | 45 | 2,99 |  |
| 82 | 4035/1 | **10** | z-fold pack | 104х100х300 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Siemens Cardiostat 31, 31S, etc. | 42 | 3,12 |  |
| 83 | 4035/2 | **10** | z-fold pack | 104х100х180 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** | 150 | 1,87 |  |
| 84 | 4036 | **2** | roll | 110х30 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** Bioset3500 , ECG Geolink, EC12Т-01-«R-D», HeartScreen 12D, Medinov ECG-9806 , etc. | 55 | 3,30 |  |
| 85 | 4036/1 | **4** | roll | 110х30 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** Bioset 3500, Geolink, EC12Т-01-«R-D», Hear tScreen 12D, Alton-038/06, Medinov ECG-9806 , etc. | 55 | 3,30 |  |
| 86 | 4036/2 | **4** | roll | 110х25 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** Bioset 3500, Geolink, ECG 3 can Ucard 200 , etc. | 63 | 2,75 |  |
| 87 | 4036/3 | **2** | roll | 110х25 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** Bioset 3500, Geolink, ECG 3 canals , etc. | 63 | 2,75 |  |
| 88 | 4036/4 | **2** | roll | 110х20 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | ECG | 72 | 2,20 |  |
| 89 | 4036/5 | **4** | roll | 110х50 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | ECG | 30 | 5,50 |  |
| 90 | 4036/6 | **4** | roll | 110х15 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** Alton-06, etc. | 100 | 1,65 |  |
| 91 | 4036/7 | **2** | roll | 110х15 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** EC12Т01-«R-D» , etc. | 100 | 1,65 |  |
| 92 | 4037 | **2** | roll | 110х30 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** Nihon Kohden, HeartScreen, etc. | 50 | 3,30 |  |
| 93 | 4037/1 | **4** | roll | 110х30 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | ECG | 50 | 3,30 |  |
| 94 | 4038 | **4** | roll | 108х23 | 16 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** Marquette, Mortara 100, etc. | 66 | 2,48 |  |
| 95 | 4038/1 | **10** | z-fold pack | 108х140х250 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** Mortara ELI 150 , etc. | 28 | 3,78 |  |
| 96 | 4038/2 | **2** | z-fold pack | 108х30 | 16 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** Mortara ELI 150 , etc. | 51 | 3,24 |  |
| 97 | 4039 | **10** | z-fold pack | 110х100х200 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Bioset 3600/3700/3601, etc. | 50 | 2,20 |  |
| 98 | 4040 | **12** | z-fold pack | 110х140х142 |  | No |  | Yes |  | Thermal paper | 55 | **ECG** Nihon Kohden, **Cardiofax** 1250К  **pacemaker** «Uni-2» , etc. | 52 | 2,19 |  |
| 99 | 4040/1 | **12** | z-fold pack | 110х140х145 |  | No |  | Yes |  | Thermal paper | 55 | **ECG** | 52 | 2,23 |  |
| 100 | 4041 | **12** | z-fold pack | 110х150х300 |  | No |  | Yes |  | Thermal paper | 55 | **ECG** NihonKohden,  **electromyograph** Neuropack 2 , etc. | 44 | 4,95 |  |
| 101 | 4042 | **8** | roll | 110х30 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment**  **Spirometer** SP 3000-SP 5000,  **Sinuscope**, Angiodin -LOR/P, Biotronik, Olympus , etc. | 55 | 3,30 |  |
| 102 | 4042/1 | **8** | roll | 110х12 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment**  **Spirometer** Microlab, etc. | 120 | 1,32 |  |
| 103 | 4042/2 | **8** | roll | 110х25 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** | 63 | 2,75 |  |
| 104 | 4042/3 | **8** | roll | 110х5 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment**  **Spirometer** Microlab, etc. | 200 | 0,55 |  |
| 105 | 4042/4 | **8** | roll | 110х20 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment**  **Spirometer** Spirolab , etc. | 90 | 2,20 |  |
| 106 | 4042/2 | **8** | roll | 110х60 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** | 25 | 6,6 |  |
| 107 | 4042/2 | **8** | roll | 110х50 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** | 30 | 5,5 |  |
| 108 | 4042/2 | **8** | roll | 110х110 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** | 12 | 12,1 |  |
| 109 | 4043 | **2** | roll | 112х27 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** Geoling, Cardico 302, EC-ZТ-02 «Aksion» , etc. | 63 | 3,02 |  |
| 110 | 4043/1 | **4** | roll | 112х27 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** Dixion 1006, Kenz-Cardico 302 , etc. | 63 | 3,02 |  |
| 111 | 4043/2 | **4** | roll | 112х30 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** KENZ, , etc. | 55 | 3,36 |  |
| 112 | 4043/3 | **8** | roll | 112х30 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** Cobas C111 etc. | 55 | 3,36 |  |
| 113 | 4043/4 | **2** | roll | 112х30 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** Kaden ECG-923A, etc. | 50 | 3,36 |  |
| 114 | 4043/5 | **4** | roll | 112х25 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** BTL-08 M-lines, etc. | 63 | 2,80 |  |
| 115 | 4043/6 | **2** | roll | 112х25 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** | 61 | 2,80 |  |
| 116 | 4043/7 | **2** | roll | 112х25 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** | 63 | 2,80 |  |
| 117 | 4044 | **10** | z-fold pack | 112х100х300 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Cardioline Delta 3+ , etc. | 35 | 3,36 |  |
| 118 | 4044/1 | **9** | z-fold pack | 112х100х160 |  | Yes |  | No mark |  | Thermal paper | 55 | **Fetal monitor** FM Lateo F 500, etc. | 60 | 1,79 |  |
| 119 | 4044/2 | **9** | z-fold pack | 112х100х150 |  | Yes |  | No mark |  | Thermal paper | 55 | **Fetal monitor** FM Bestman BV 610, etc. | 60 | 1,68 |  |
| 120 | 4044/3 | **13** | z-fold pack | 112х100х150 |  | Yes |  | Yes, on the back |  | Thermal paper | 55 | **Fetal monitor** FM Sunray, etc. | 60 | 1,68 |  |
| 121 | 4044/4 | **13** | z-fold pack | 112х100х150 |  | Yes |  | Yes, on the back |  | Thermal paper | 55 | **Fetal monitor** FMGOLDWAY, UT 3000 A, ECG 1206 D , etc. | 60 | 1,68 |  |
| 122 | 4044/5 | **9** | z-fold pack | 112х100х150 |  | Yes |  | No mark |  | Thermal paper | 55 | **Fetal monitor** FMCTG 6A, etc. | 60 | 1,68 |  |
| 123 | 4045 | **9** | z-fold pack | 116х120х250 |  | Yes |  | No mark |  | Thermal paper | 55 | **Fetal monitor** FM Analogic, **Cardiotocograph** CTG Sonicaid Team, etc. | 36 | 3,48 |  |
| 124 | 4046 | **3** | roll | 120х30 | 19 | Yes | outward | Yes |  | Thermal paper | 55 | **ECG** Cardioline ETA 3, CardietteExel, Cardiorapid, Bohse, Doctor Lee ECG-310A, etc. | 48 | 3,60 |  |
| 125 | 4046/1 | **8** | roll | 120х30 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment biochemical analyzer**, etc. | 50 | 3,60 |  |
| 126 | 4046/2 | **3** | roll | 120х20 | 19 | Yes | outward | Yes |  | Thermal paper | 55 | **ECG** Cardiette AR 1200, etc. | 63 | 2,40 |  |
| 127 | 4046/3 | **10** | z-fold pack | 120х100х200 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Cardiette AR 1200, etc. | 68 | 2,40 |  |
| 128 | 4046/4 | **10** | z-fold pack | 120х100х300 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Cardiette AR 1200, etc. |  | 3,60 |  |
| 129 | 4046/5 | **6** | roll | 120х30 | 12 | No | inward | No mark |  | Thermal paper | 55 | **Laboratory equipment** | 50 | 3,60 |  |
| 130 | 4047 | **9** | z-fold pack | 120х100х150 |  | Yes |  | No mark |  | Thermal paper | 55 | **Fetal monitor** FM Advanced AM-66, Kontron AN 66, FM Photoscan , etc. | 70 | 1,80 |  |
| 131 | 4047/1 | **9** | z-fold pack | 120х120х250 |  | Yes |  | No mark |  | Thermal paper | 55 | **Fetal monitor** FM Biosys IFM 500, etc. | 60 | 3,60 |  |
| 132 | 4048 | **10** | z-fold pack | 126х150х170 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Biomedica Personal C 120, etc. | 60 | 3,21 |  |
| 133 | 4049 | **3** | roll | 130х25 | 16 | Yes | outward | Yes |  | Thermal paper | 55 | **ECG** CardietteStart 100, etc. | 50 | 3,25 |  |
| 134 | 4050 | **2** | roll | 130х30 | 20 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** CardisunyFucuda 503A, etc. | 46 | 3,90 |  |
| 135 | 4051 | **10** | z-fold pack | 130х135х370 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Hellige EK 53/56,Cardioline, etc. | 19 | 6,49 |  |
| 136 | 4052 | **10** | z-fold pack | 135х140х150 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Schiller AT-5, etc. | 52 | 2,83 |  |
| 137 | 4053 | **10** | z-fold pack | 112х90х300 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** KENZ 302, etc. | 42 | 3,02 |  |
| 138 | 4054 | **2** | roll | 145х30 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** Fucuda, Nihon Kohden ,Siemens Sicard 440, Cardimax FX-8222, etc. | 40 | 4,35 |  |
| 139 | 4054/1 | **4** | roll | 145х30 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** Fucuda, Nihon Kohden , etc. | 40 | 4,35 |  |
| 140 | 4054/2 | **2** | roll | 143х30 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** | 40 | 4,29 |  |
| 141 | 4054/3 | **2** | roll | 145х30 | 16 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** Fucuda, Nihon Kohden , etc. | 42 | 4,35 |  |
| 142 | 4054/4 | **2** | roll | 143х30 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** Bosh, etc. | 40 | 4,29 |  |
| 143 | 4054/5 | **4** | roll | 145х30 | 16 | Yes | outward | No mark |  | Thermal paper | 55 | ECG | 40 | 4,35 |  |
| 144 | 4054/6 | **4** | roll | 145х30 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | ECG | 40 | 4,35 |  |
| 145 | 4054/7 | **3** | roll | 145х60 | 18 | Yes | outward | Yes |  | Thermal paper | 55 | ECG | 20 | 8,70 |  |
| 146 | 4054/8 | **4** | roll | 145х60 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | ECG | 20 | 8,70 |  |
| 147 | 4054/9 | **9** | z-fold pack | 145х75х267 |  | Yes |  | No mark |  | Thermal paper | 55 | **ECG** Fukuda FX 8222 , etc. | 42 | 2.9 |  |
| 148 | 4055 | **10** | z-fold pack | 145х100х350 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Schiller AT-6 , etc. | 24 | 5,08 |  |
| 149 | 4056 | **13** | z-fold pack | 145х100х250 |  | Yes |  | Yes, on the back |  | Thermal paper | 55 | **ECG** Nihon Kohden, FQS 145-2/5-100 , etc. | 35 | 3,62 |  |
| 150 | 4057 | **13** | z-fold pack | 148х100х400 |  | Yes |  | Yes, on the back |  | Thermal paper | 55 | **ECG** Siemens Sicard 460 , etc. | 24 | 5,92 |  |
| 151 | 4057/1 | **3** | roll | 148х25 | 18 | Yes | outward | Yes, on the back |  | Thermal paper | 55 | **ECG** Siemens Sicard 460, etc. | 48 | 3,7 |  |
| 152 | 4058 | **10** | z-fold pack | 150х100х150 |  | Yes |  | Yes |  | Thermal paper | 55 | **Fetal monitor** Hewlett-Packard M 1911 HP M 1911/M 1351 FM Phillips, Avalon, etc. | 70 | 2,25 |  |
| 153 | 4058/1 | **11** | z-fold pack | 150х150х200 |  | No |  | No mark |  | Thermal paper | 55 | **Fetal monitor** FM Kranzbuhler (BabyDoplex) , etc. | 40 | 4,50 |  |
| 154 | 4058/2 | **14** | z-fold pack | 151х100х150 |  | Yes |  | Yes, two marks |  | Thermal paper | 55 | **Fetal monitor** FM Hewlett-Packard М 1910 А, Dixion Overton 6200, etc. | 60 | 2,26 |  |
| 155 | 4059 | **9** | z-fold pack | 152х150х200 |  | Yes |  | No mark | Yes, on two sides | Thermal paper | 55 | **Fetal monitor** Toitu, FM, etc. | 36 | 4,56 |  |
| 156 | 4060 | **2** | roll | 170х50 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** 4-canals. ECG, EC - 4Т, etc. | 20 | 8,50 |  |
| 157 | 4061 | **2** | roll | 183х30 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** Kenz, Siemens, Hellige , etc. | 34 | 5,49 |  |
| 158 | 4061/1 | **4** | roll | 183х30 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | ECG | 34 | 5,49 |  |
| 159 | 4062 | **2** | roll | 210х30 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** Bioset 8000, ECG Dixion 1012, etc. | 26 | 6,30 |  |
| 160 | 4062/1 | **6** | roll | 210х30 | 12 | No | inward | No mark |  | Thermal paper | 55 | **ECG** Nihon Kohden 1350, etc. | 26 | 6,30 |  |
| 161 | 4062/2 | **4** | roll | 210х30 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** Вioset 8000, Bionet Cardico Care2000, Kaden 9012, etc. | 26 | 6,30 |  |
| 162 | 4062/3 | **8** | roll | 210х25 | 12 | No | outward | No mark |  | Thermal paper | 55 | **ECG** BTL-08-M lines, etc. | 26 | 5,25 |  |
| 163 | 4063 | **2** | roll | 210х30 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** 6 canals Fukuda FCP 4101, Fukuda Cardimax FX 8322R, Cardimax FX 7402, Nihon Kohden 1350, Medinova 9812, etc. | 25 | 6,30 |  |
| 164 | 4063/1 | **4** | roll | 210х30 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** 4 canals , EC 4Т, Sensitec ECG 1012, etc. | 25 | 6,30 |  |
| 165 | 4063/2 | **9** | z-fold pack | 210х100х140 |  | Yes |  | No mark |  | Thermal paper | 55 | **ECG** Fukuda Cardimax FX 7402, etc. | 42 | 2,94 |  |
| 166 | 4063/3 | **4** | roll | 210х25 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | ECG | 25 | 5,25 |  |
| 167 | 4063/4 | **2** | roll | 210х20 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | ECG | 30 | 4,2 |  |
| 168 | 4064 | **3** | roll | 210х30 | 20 | Yes | outward | Yes |  | Thermal paper | 55 | **ECG** Cardiette Dedalus, etc. | 25 | 6,3 |  |
| 169 | 4064/2 | **3** | roll | 210х30 | 18 | Yes | outward | Yes |  | Thermal paper | 55 | **ECG** Cardiette Dedalus, etc.. | 25 | 6,30 |  |
| 170 | 4064/3 | **1** | roll | 210х20 | 18 | Yes | inward | Yes |  | Thermal paper | 55 | **ECG** Cardiette Dedalus, etc. | 30 | 4,20 |  |
| 171 | 4064/4 | **3** | roll | 210х20 | 18 | Yes | outward | Yes |  | Thermal paper | 55 | **ECG** Cardiette Dedalus, etc. | 30 | 4,20 |  |
| 172 | 4065 | **10** | z-fold pack | 210х140х250 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Schiller AT-10 , etc. | 18 | 7,35 |  |
| 173 | 4065/1 | **10** | z-fold pack | 207х135х370 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Hellige ЕК 512, etc. | 13 | 10,34 |  |
| 174 | 4065/2 | **10** | z-fold pack | 210х140х160 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** Schiller AT-10 plus , Sensitec ECG 1012 , etc. | 20 | 4,70 |  |
| 175 | 4065/3 | **10** | z-fold pack | 210х140х140 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Schiller AT-10 , etc. | 30 | 4,12 |  |
| 176 | 4065/4 | **10** | z-fold pack | 210х140х215 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Schiller AT-10 , , etc. | 23 | 6,32 |  |
| 177 | 4066 | **10** | z-fold pack | 210х140х140 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Biocare 1230, Edan, etc. | 30 | 4,12 |  |
| 178 | 4067 | **10** | z-fold pack | 210х150х170 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Biomedica C-210, etc. | 28 | 5,36 |  |
| 179 | 4068 | **12** | z-fold pack | 210х150х280 |  | No |  | Yes |  | Thermal paper | 55 | **ECG** Biomedica Р 80 , etc. | 12 | 8,82 |  |
| 180 | 4069 | **10** | z-fold pack | 210х150х200 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Burdick Eclipse 800/850, etc. | 22 | 6,30 |  |
| 181 | 4070 | **10** | z-fold pack | 210х280х215 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Schiller AT-2, AT-2 plus, CS 200 , etc. | 10 | 12,64 |  |
| 182 | 4070/1 | **10** | z-fold pack | 210х280х215 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** Schiller AT-2, AT-2 plus. , etc. | 8 | 12,64 |  |
| 183 | 4070/2 | **10** | z-fold pack | 210х280х173 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** Schiller AT-102, AT-102 plus, AT 102 C , etc. | 10 | 10,17 |  |
| 184 | 4070/3 | **10** | z-fold pack | 210х280х360 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Schiller AT-2, AT-2 plus, , etc. | 6 | 21,17 |  |
| 185 | 4070/4 | **10** | z-fold pack | 210х280х200 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** Schiller AT-2 , etc. | 9 | 11,76 |  |
| 186 | 4071 | **9** | z-fold pack | 210х300х200 |  | Yes |  | No mark | Yes | Thermal paper | 70 | **ECG** Burdick 350, Megacart 150 E, Simens Sicard 740 , etc. | 8 | 12,60 |  |
| 187 | 4071/1 | **10** | z-fold pack | 210х300х200 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** Burdick QuestSpecelabs, etc. | 9 | 12,60 |  |
| 188 | 4072 | **10** | z-fold pack | 210х300х200 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Biomedica Archimed , etc. | 11 | 12,60 |  |
| 189 | 4073 | **13** | z-fold pack | 210х150х200 |  | Yes |  | Yes, on the back |  | Thermal paper | 55 | **ECG** Fucuda Alpha 2000 , etc. | 22 | 6,30 |  |
| 190 | 4073/1 | **13** | z-fold pack | 210х150х200 |  | Yes |  | Yes, on the back |  | Thermal paper | 70 | **ECG** FucudaAlpha 2000 , etc. | 16 | 6,30 |  |
| 191 | 4074 | **9** | z-fold pack | 210х300х200 |  | Yes |  | No mark | Yes | Thermal paper | 70 | **ECG** HP 1709A/1700/1701 Page Writer 200 , etc. | 9 | 12,60 |  |
| 192 | 4075 | **10** | z-fold pack | 210х150х500 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Bioset 9000, etc. | 8 | 15,75 |  |
| 193 | 4076 | **2** | roll | 250х50 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** 6 canals EC-6Т, etc. | 12 | 12,50 |  |
| 194 | 4077 | **10** | z-fold pack | 210х150х240 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Kenz 1211, etc. | 18 | 7,56 |  |
| 195 | 4077/1 | **3** | roll | 210х50 | 12 | Yes | outward | Yes |  | Thermal paper | 55 | **ECG** Kenz 1211, etc. | 14 | 10,5 |  |
| 196 | 4078 | **9** | z-fold pack | 112х120х250 |  | Yes |  | No mark |  | Thermal paper | 55 | **Fetal monitor** FM Biosys CTG BFM-800/900 (Printer Bionics) , etc. | 46 | 3,36 |  |
| 197 | 4078/1 | **4** | roll | 112х30 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **Fetal monitor** FM Biosys CTG BFM-800/900 (Printer Bionics) , etc. | 55 | 3,36 |  |
| 198 | 4079 | **4** | roll | 106х22 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **Defibrillator** Corpuls-3, etc. | 65 | 2.33 |  |
| 199 | 4079/1 | **4** | roll | 106х22 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | **Defibrillator** Corpuls-3, etc. | 60 | 2.33 |  |
| 200 | 4079/2 | **4** | roll | 106,5х22 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | **Defibrillator** Corpuls-3, etc. | 60 | 2.34 |  |
| 201 | 4079/3 | **8** | roll | 106х22 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Defibrillator** Corpuls-3, etc. | 70 | 2.33 |  |
| 202 | 4080 | **8** | roll | 69х40 | 12 | No |  | No mark |  | Chart (diagram) paper | 50 | **Laboratory equipment** | 48 | 2,76 |  |
| 203 | 4081 | **4** | roll | 55х30 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | ECG | 72 | 1,65 |  |
| 204 | 4081/1 | **4** | roll | 55х25 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | ECG | 80 | 1,38 |  |
| 205 | 4081/2 | **2** | roll | 55х25 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | ECG | 80 | 1,38 |  |
| 206 | 4081/3 | **4** | roll | 55х30 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | ECG | 64 | 1,65 |  |
| 207 | 4081/4 | **2** | roll | 55х30 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | ECG | 64 | 1,65 |  |
| 208 | 4081/5 | **8** | roll | 55х40 | 16 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** | 48 | 2,20 |  |
| 209 | 4081/6 | **2** | roll | 55х20 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | ECG | 84 | 1,10 |  |
| 210 | 4081/7 | **2** | roll | 55х20 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | ECG | 84 | 1,10 |  |
| 211 | 4081/8 | **4** | roll | 55х20 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | ECG | 84 | 1,10 |  |
| 212 | 4081/9 | **4** | roll | 55х50 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | ECG | 40 | 2,75 |  |
| 213 | 4082 | **2** | roll | 151х24 | 16 | Yes | inward | No mark |  | Thermal paper | 55 | **Fetal monitor** FM BIONET FC 1400 , etc. | 46 | 3,62 |  |
| 214 | 4082/1 | **2** | roll | 150х25 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **Fetal monitor** FM BIONET FC 1400, etc. | 46 | 3,75 |  |
| 215 | 4082/2 | **4** | roll | 150х25 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | **Fetal monitor** FM BIONET FC 1400, etc. | 46 | 3,75 |  |
| 216 | 4083 | **3** | roll | 216х60 | 18 | Yes | outward | Yes |  | Thermal paper | 55 | **ECG** Nihon Kohden, etc. | 12 | 12,96 |  |
| 217 | 4083/1 | **8** | roll | 216х50 | 12 | No | outward | No mark |  | Thermal paper | 55 | **ECG** Nihon Kohden, etc. | 14 | 10,80 |  |
| 218 | 4084 | **13** | z-fold pack | 145х150х400 |  | Yes |  | Yes, on the back |  | Thermal paper | 55 | **ECG** Siemens Cardiostat 3, Fucuda Alpha-600/C 300, etc. | 20 | 8,70 |  |
| 219 | 4085 | **13** | z-fold pack | 63х100х500 |  | Yes |  | Yes, on the back |  | Thermal paper | 55 | **ECG** Fukuda, Alphа 501 AX, Fukuda, Alphа 1000, Cardiosunny, etc. | 32 | 3,15 |  |
| 220 | 4086 | **10** | z-fold pack | 210х280х200 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** BiomedikaPower 80, Schiller АТ-102, etc. | 11 | 11,76 |  |
| 221 | 4086/1 | **10** | z-fold pack | 210х280х200 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** Welch Allyn CP-100 , etc. | 9 | 11,76 |  |
| 222 | 4086/2 | **10** | z-fold pack | 210х280х143 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Shiller AT-102, etc. | 16 | 8,41 |  |
| 223 | 4087 | **3** | roll | 210х30 | 12 | Yes | outward | Yes, along the rim |  | Thermal paper | 55 | **ECG** Bioset 8000, etc. | 26 | 6,30 |  |
| 224 | 4087/1 | **8** | roll | 215х25 | 18 | No | outward | No mark |  | Thermal paper | 55 | **ECG** | 27 | 5,38 |  |
| 225 | 4087/2 | **2** | roll | 215х20 | 20 | Yes | inward | No mark |  | Thermal paper | 55 | **Fetal monitor** FM Bionet FC 700, etc. | 23 | 4,30 |  |
| 226 | 4087/18 | **4** | roll | 215х25 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | **Fetal monitor** FM Bionet FC 700, etc. | 27 | 5,37 |  |
| 227 | 4087/3 | **4** | roll | 216х30 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** Cardipia 800, etc. | 25 | 6,48 |  |
| 228 | 4087/4 | **2** | roll | 216х30 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** Cardipia 800, etc. | 25 | 6,48 |  |
| 229 | 4087/5 | **4** | roll | 215х20 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | **Fetal monitor** FM Bionet FC 700, etc. | 23 | 4,30 |  |
| 230 | 4087/6 | **2** | roll | 215х20 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **Fetal monitor** FM Bionet FC 700, etc. | 23 | 4,30 |  |
| 231 | 4087/7 | **2** | roll | 215х25 | 18 | Yes | inward | No mark |  | Thermal paper | 55 | **Fetal monitor** FM Bionet FC 700, etc. | 27 | 5,40 |  |
| 232 | 4087/8 | **4** | roll | 215х30 | 18 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** |  | 6,45 |  |
| 233 | 4087/9 | **6** | roll | 215х30 | 18 | No | inward | No mark |  | Thermal paper | 55 | **Laboratory equipment** |  | 6,45 |  |
| 234 | 4087/10 | **8** | roll | 215х30 | 18 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** |  | 6,45 |  |
| 235 | 4088 | **10** | z-fold pack | 215х280х200 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** Mediana YM 8121 , etc. |  | 12,04 |  |
| 236 | 4089 | **12** | z-fold pack | 210х140х300 |  | No |  | Yes |  | Thermal paper | 55 | **ECG** NihonKohden 9130, Dixion ECG 1012, etc. | 14 | 8,82 |  |
| 237 | 4089/1 | **12** | z-fold pack | 210х140х215 |  | No |  | Yes |  | Thermal paper | 55 | **ECG** Nihon Kohden FQW 210, Dixion ECG 1012-3-140, etc. | 20 | 6,32 |  |
| 238 | 4091/1 | **10** | z-fold pack | 210х300х250 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** EC Mortara ELI 250 , etc. | 7 | 15,75 |  |
| 239 | 4091/2 | **3** | roll | 210х22 | 12 | Yes | outward | Yes |  | Thermal paper | 55 | **ECG** EC Mortara ELI 250 , etc. |  | 4,62 |  |
| 240 | 4091/3 | **8** | roll | 210х70 | 18 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** |  | 14,7 |  |
| 241 | 4092 | **2** | roll | 140х43 | 20 | Yes | inward | No mark |  | Thermal paper | 55 | Cardiotocograph, etc. | 24 | 6,02 |  |
| 242 | 4092/1 | **7** | roll | 104х15 | 12 | No | outward | Yes |  | Thermal paper | 55 | **Laboratory equipment** | 76 | 2,1 |  |
| 243 | 4093 | **10** | z-fold pack | 210х280х360 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Schiller АТ-60,Fukuda, etc. | 6 | 21,17 |  |
| 244 | 4094 | **8** | roll | 50х20 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment biochemical analyzer** Mindray ВС-300+, etc. | 130 | 1,00 |  |
| 245 | 4094/1 | **2** | roll | 50х30 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | **ECG** KENZ 108, ECOR, Biocare ECG-101G, etc. | 85 | 1,50 |  |
| 246 | 4094/2 | **8** | roll | 50х23 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment biochemical analyzer**, etc. | 98 | 1,15 |  |
| 247 | 4094/3 | **8** | roll | 50х30 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment biochemical analyzer, defibrillator**, etc. | 85 | 1,50 |  |
| 248 | 4094/4 | **4** | roll | 50х30 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** Medinova 9801, etc. | 85 | 1,50 |  |
| 249 | 4094/5 | **8** | roll | 50х50 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** | 48 | 2,50 |  |
| 250 | 4094/6 | **6** | roll | 50х50 | 12 | No | inward | No mark |  | Thermal paper | 55 | **Laboratory equipment** Analyzer ВС-3000 plusMindray, etc. | 48 | 2,50 |  |
| 251 | 4094/7 | **2** | roll | 50х50 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | **Laboratory equipment** | 48 | 2,50 |  |
| 252 | 4094/8 | **6** | roll | 50х20 | 12 | No | inward | No mark |  | Thermal paper | 55 | **Laboratory equipment biochemical analyzer, etc.** | 162 | 1,00 |  |
| 253 | 4094/9 | **4** | roll | 50х50 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** | 48 | 2,50 |  |
| 254 | 4094/10 | **4** | roll | 50х20 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** | 105 | 1,00 |  |
| 255 | 4094/11 | **8** | roll | 50х25 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** | 105 | 1,25 |  |
| 256 | 4094/12 | **2** | roll | 50х20 | 12 | Yes | inward | No mark |  | Thermal paper | 55 | **Laboratory equipment** | 105 | 1,00 |  |
| 257 | 4094/13 | **6** | roll | 50х30 | 12 | No | inward | No mark |  | Thermal paper | 55 | **Laboratory equipment** | 85 | 1,5 |  |
| 258 | 4094/14 | **8** | roll | 50х42 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** |  | 2,1 |  |
| 259 | 4094/15 | **4** | roll | 50х23 | 12 | Yes | outward | No mark |  | Thermal paper | 55 | **ECG** | 98 | 1,15 |  |
| 260 | 4094/16 | **8** | roll | 50х10 | 12 | No | outward | No mark |  | Thermal paper | 55 | **Laboratory equipment** |  | 0,5 |  |
| 261 | 4095 | **14** | z-fold pack | 150х90х150 |  | Yes |  | Yes, two marks |  | Thermal paper | 55 | **Fetal monitor** FM Comen Star 5000 F; 5000 D , etc. | 70 | 2,02 |  |
| 262 | 4096 | **14** | z-fold pack | 152х90х150 |  | Yes |  | No mark |  | Thermal paper | 55 | **Fetal monitor** FM Corometrics 4305 BAO, Dixion 6900, FM G6B (General Meditech), Analogic Fetalgard lite, etc. | 70 | 2,05 |  |
| 263 | 4096/1 | **9** | z-fold pack | 152х90х160 |  | Yes |  | No mark |  | Thermal paper | 55 | **Fetal monitor** FM Bistos/Corometrics 4305 AAO/CAO, Corometrics -170, Bistos BT-350, МеdianaFM-20, G6 Bplus ; FM Edan F9, etc. | 70 | 2,19 |  |
| 264 | 4096/2 | **9** | z-fold pack | 152х100х160 |  | Yes |  | No mark |  | Thermal paper | 55 | **Fetal monitor** FM Neoventa STAN S31, etc. | 70 | 2,43 |  |
| 265 | 4097 | **10** | z-fold pack | 110х140х142 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** FukudaDenshi FX7202, FukudaCardimax, FX-8322 Medinov ECG-9806, DixionECG 1006, etc. | 52 | 2,19 |  |
| 266 | 4097/1 | **10** | z-fold pack | 110х140х145 |  | Yes |  | Yes |  | Thermal paper | 55 | ECG | 52 | 2,23 |  |
| 267 | 4097/2 | **10** | z-fold pack | 110х140х150 |  | Yes |  | Yes |  | Thermal paper | 55 | ECG | 52 | 2.31 |  |
| 268 | 4098 | **10** | z-fold pack | 110х140х200 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** MAC-800 , etc. | 35 | 3,08 |  |
| 269 | 4099 | **3** | roll | 60х15 | 16 | Yes | outward | Yes |  | Thermal paper | 55 | **ECG** Cardietta АR600, Cardioline, etc. | 96 | 0,90 |  |
| 270 | 4099/1 | **10** | z-fold pack | 60х75х250 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Cardietta AR 600, etc. | 90 | 1,13 |  |
| 271 | 4100 | **13** | z-fold pack | 145х125х240 |  | Yes |  | Yes, on the back |  | Thermal paper | 55 | **ECG** NecKartizer 3321, etc. | 36 | 4,35 |  |
| 272 | 4101 | **9** | z-fold pack | 50х100х300 |  | Yes |  | No mark |  | Thermal paper | 55 | Defibrillator NK TEC 7721K, etc. | 84 | 1,50 |  |
| 273 | 4102 | **10** | z-fold pack | 183х130х200 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Kenz 1207, etc. | 24 | 4,76 |  |
| 274 | 4103 | **10** | z-fold pack | 114х70х250 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG -** CP50 WelchAllyn, etc. | 48 | 2,00 |  |
| 275 | 4104 | **10** | z-fold pack | 90х90х360 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Mac-500, Hellige, etc. | 40 | 2,91 |  |
| 276 | 4104/1 | **10** | z-fold pack | 90х90х360 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** Mac-500, Hellige, etc. | 30 | 2,91 |  |
| 277 | 4105 | **9** | z-fold pack | 130х120х250 |  | Yes |  | No mark |  | Thermal paper | 55 | **Fetal monitor** FM Bistos (CTG) , etc. | 28 | 3,90 |  |
| 278 | 4106 | **13** | z-fold pack | 112х90х150 |  | Yes |  | Yes, on the back |  | Thermal paper | 55 | **Fetal monitor** FM Dixion Overton 6100, Comen Star 5000, 5000С, CTGG6A-plus, «Dafina» BF 610P, etc. | 80 | 1,51 |  |
| 279 | 4106/1 | **9** | z-fold pack | 112х90х122 |  | Yes |  | No mark |  | Thermal paper | 55 | **Fetal monitor** FM Cadence 240, etc. | 100 | 1,23 |  |
| 280 | 4107 | **10** | z-fold pack | 112х150х300 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** HeartScreen, etc. | 30 | 5,04 |  |
| 281 | 4107/1 | **12** | z-fold pack | 112х150х300 |  | No |  | Yes |  | Thermal paper | 55 | **Programmer** Orchestra plus, etc. | 30 | 5,04 |  |
| 282 | 4108 | **9** | z-fold pack | 120х40х400 |  | Yes |  | No mark |  | Thermal paper | 55 | **Laboratory equipment sterilizer** Getinge, etc. | 70 | 1,92 |  |
| 283 | 4108/1 | **9** | z-fold pack | 120х40х240 |  | Yes |  | No mark |  | Thermal paper | 55 | **Laboratory equipment sterilizer** Getinge, etc. | 100 | 1,15 |  |
| 284 | 4160 | **10** | z-fold pack | 210х300х150 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** MAC-1200 , etc. | 14 | 9,45 |  |
| 285 | 4160/0 | **10** | z-fold pack | 210х300х150 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** MAC-1200 , etc. | 11 | 9,45 |  |
| 286 | 4160/1 | **10** | z-fold pack | 210х295х150 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** MAC-1200 ST , MAC-1600 , etc. | 12 | 9,29 |  |
| 287 | 4161 | **10** | z-fold pack | 216х280х250 |  | Yes |  | Yes |  | Thermal paper | 75 | **ECG** MortaraRangoni ELI 350 , etc. | 6 | 15,12 |  |
| 288 | 4162 | **15** | z-fold pack | 210х280х300 |  | Yes |  | No mark | Yes | Thermal paper | 70 | **ECG** Marquette, MAC 1-6,12-15 , etc. | 6 | 18,14 |  |
| 289 | 4163 | **10** | z-fold pack | 210х150х320 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** KENZ 1210, etc. | 12 | 10,08 |  |
| 290 | 4163/1 | **10** | z-fold pack | 210х150х240 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** KENZ 1210, etc. | 18 | 7,56 |  |
| 291 | 4164 | **10** | z-fold pack | 80х70х315 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Schiller АТ-101 , etc. | 60 | 1,76 |  |
| 292 | 4164/1 | **10** | z-fold pack | 80х70х275 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Schiller АТ-101, etc. | 70 | 1,54 |  |
| 293 | 4164/2 | **10** | z-fold pack | 80х70х300 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** Schiller АТ-101 , etc. | 45 | 1,68 |  |
| 294 | 4164/3 | **10** | z-fold pack | 80х70х315 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** Schiller АТ-101, etc. | 45 | 1,76 |  |
| 295 | 4164/4 | **10** | z-fold pack | 80х70х300 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Schiller АТ-101 , etc. | 45 | 1,68 |  |
| 296 | 4164/5 | **10** | z-fold pack | 80х70х275 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** Schiller АТ-101 , etc. | 54 | 1,54 |  |
| 297 | 4165 | **10** | z-fold pack | 210х150х200 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** Dedalus K 600D/AR2100 , etc. | 18 | 6,30 |  |
| 298 | 4165/1 | **10** | z-fold pack | 210х280х200 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** Cardioline AR 2100 view , etc. | 8 | 11,76 |  |
| 299 | 4166 | **15** | z-fold pack | 210х145х200 |  | Yes |  | No mark | Yes | Thermal paper | 55 | **ECG** BionetCardico XP, etc. | 22 | 6,09 |  |
| 300 | 4166/1 | **15** | z-fold pack | 210х145х200 |  | Yes |  | No mark | Yes | Thermal paper | 70 | **ECG** BionetCardico XP , etc. | 18 | 6,09 |  |
| 301 | 4167 | **10** | z-fold pack | 210х150х200 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Schiller SC-6/12, etc. | 22 | 6,30 |  |
| 302 | 4167/1 | **10** | z-fold pack | 210х150х400 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Schiller SC-6/12, etc. | 10 | 12,6 |  |
| 303 | 4168 | **12** | z-fold pack | 143х150х300 |  | No |  | Yes |  | Thermal paper | 55 | **Fetal monitor** FM Oxford, Sonicaid, Meridian 800, ТЕАМ 8003, 8400-8300, etc. | 20 | 6,43 |  |
| 304 | 4181 | **10** | z-fold pack | 210х295х400 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** Dixion 6 can. , etc. | 4 | 24,78 |  |
| 305 | 4181/1 | **10** | z-fold pack | 210х295х150 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** Dixion 6 can. , etc. | 12 | 9,29 |  |
| 306 | 4181/2 | **10** | z-fold pack | 210х295х340 |  | Yes |  | Yes |  | Thermal paper | 70 | **ECG** Dixion 6 can. , etc. | 5 | 21,06 |  |
| 307 | 4182 | **12** | z-fold pack | 210х295х215 |  | No |  | Yes |  | Thermal paper | 55 | **ECG** Nihon Kohden, etc. | 10 | 13,32 |  |
| 308 | 4182/1 | **12** | z-fold pack | 210х295х340 |  | No |  | Yes |  | Thermal paper | 55 | **ECG** Nihon Kohden, etc. |  | 21.06 |  |
| 309 | 4183 | **9** | z-fold pack | 80х80х200 |  | Yes |  | No mark |  | Thermal paper | 55 | **Defibrillator** Primedic EVO, etc. | 80 | 1,28 |  |
| 310 | 4195 | **10** | z-fold pack | 114х95х140 |  | Yes |  | Yes |  | Thermal paper | 55 | **ECG** Schiller MS-2007, etc. | 75 | 1,51 |  |
| 311 | 4196 | **8** | roll | 49х30 | 12 | No | outward | No mark |  | Thermal paper | 55 | Laboratory equipment | 80 | 1,47 |  |
| 312 | 4196/1 | **8** | roll | 49х45 | 12 | No | outward | No mark |  | Thermal paper | 55 | Laboratory equipment | 46 | 2,2 |  |
| 313 | 4197 | **8** | roll | 37х10 | 12 | No | outward | No mark |  | Thermal paper | 55 | Laboratory equipment | 100 | 0,37 |  |
| 314 | 4197/1 | **8** | roll | 37х20 | 12 | No | outward | No mark |  | Thermal paper | 55 | Laboratory equipment | 144 | 0,74 |  |
| 315 | 4197/2 | **8** | roll | 37х15 | 12 | No | outward | No mark |  | Thermal paper | 55 | Laboratory equipment | 120 | 0,56 |  |
| 316 | 4198 | **8** | roll | 76х25 | 12 | No | outward | No mark |  | Thermal paper | 55 | Laboratory equipment | 65 | 1,9 |  |
| 317 | 4199 | **8** | roll | 56х30 | 12 | No | outward | No mark |  | Thermal paper | 55 | Laboratory equipment | 72 | 1,68 |  |
| 318 | 4200 | **8** | roll | 72х25 | 12 | No | outward | No mark |  | Thermal paper | 55 | Laboratory equipment | 65 | 1,8 |  |
| 319 | 5001 | **9** | z-fold pack | 240х300х500 |  | Yes |  | No mark |  | Chart (diagram) paper | 50 | **Electroencephalograph** EEG Biospirt,  **Geoanalyzer** «Micros» , etc. | 3 | 36,00 |  |
| 320 | 5002 | **9** | z-fold pack | 245х300х1000 |  | Yes |  | No mark |  | Chart (diagram) paper | 50 | **Electroencephalograph** NihonKohden NK245F 16-can, Neurofax 7300, etc. | 1 | 73,50 |  |
| 321 | 5002/1 | **9** | z-fold pack | 300х300х500 |  | Yes |  | No mark |  | Thermal paper | 55 | **ECG** NihonKohden , etc. | 2 | 45,00 |  |
| 322 | 5002/2 | **9** | z-fold pack | 300х300х1000 |  | Yes |  | No mark |  | Thermal paper | 55 | **ECG** NihonKohden, etc. | 1 | 90,00 |  |
| 323 | 5003 | **9** | z-fold pack | 250х300х500 |  | Yes |  | No mark |  | Chart (diagram) paper | 50 | **Electroencephalograph** EEG Medicor 8Х (8С), EEG Bioscript 101, etc. | 3 | 37,50 |  |
| 324 | 5003/1 | **9** | z-fold pack | 250х150х500 |  | Yes |  | No mark |  | Chart (diagram) paper | 50 | **Electroencephalograph** EEG Medicor 8Х (8С), EEG Bioscript 101, etc. | 6 | 18,75 |  |
| 325 | 5004 | **9** | z-fold pack | 400х300х1000 |  | Yes |  | No mark |  | Chart (diagram) paper | 50 | **Electroencephalograph** EEG NihonKohden FV 400-30 (21CH), etc. | 2 | 120,00 |  |
| 326 | 5005 | **9** | z-fold pack | 345х300х1000 |  | Yes |  | No mark |  | Chart (diagram) paper | 50 | **Electroencephalograph** EEG NihonKohden 7214, NK FV345-30, NK345F 17 can,Neurofax 4400, etc. | 1 | 103,50 |  |
| 327 | 5006 | **9** | z-fold pack | 420х300х500 |  | Yes |  | No mark |  | Chart (diagram) paper | 50 | **Electroencephalograph** EEG Medicor 16S 16X, etc. | 3 | 63,00 |  |
| 328 | 5008 | **9** | z-fold pack | 250х200х500 |  | Yes |  | No mark |  | Chart (diagram) paper | 65 | **ECG** Вioset( MWZ) -6000, etc. | 3 | 25,00 |  |
| 329 | 4222 | **8** | roll | 84х13,5 | 12 | No | outward | No mark |  | Thermal film | 63 | **Printer for ultrasound equipment** Sony:UP-D711MD |  | 1,13 |  |
| 330 | 4333 | **8** | roll | 84х12,5 | 12 | No | outward | No mark |  | Thermal film | 63 | **Printer for ultrasound equipment** Sony:UP-D711MD |  | 1,05 |  |
| 331 | 4444 | **8** | roll | 105х20 | 12 | No | outward | No mark |  | Thermal film | 63 | **Printer for ultrasound equipment** Shimadzu 001-KPT | 100 | 2,1 |  |
| 332 | 4555 | **8** | roll | 210х25 | 26 | No | outward | No mark |  | Thermal film | 68 | **Printer for ultrasound equipment** Sony: UP-910, UP-930, UP-960, UP-980 etc. | 25 | 5,25 |  |
| 333 | 4777 | **8** | roll | 110х20 | 12 | No | outward | No mark |  | Thermal film | 63 | **Printer for ultrasound equipment** Sony: UP-860, UP-870, UP-890, UP-895, UP-897, UP-D860, UP-D890, UP-D895, UP-D897 and its modifications (with the letters CE, MD, MDW etc.), and also OEM-printers Aloca Ultrasound. | 100 | 2,2 |  |
| 334 | 4888 | **8** | roll | 110х20 | 12 | No | outward | No mark |  | Thermal film | 68 | **Printer for ultrasound equipment** Sony: UP-860, UP-890, UP-895, UP-897, UP-897MD, UP-D860, UP-D890, UP-D895, UP-D897, UP-X898MD etc. | 100 | 1,98 |  |
| 335 | 4999 | **8** | roll | 110х18 | 12 | No | outward | No mark |  | Thermal film | 75 | **Printer for ultrasound equipment** Sony: UP-895, UP-897, UP-D897, UP-D895 etc. | 100 | 1,98 |  |
| 336 | 3717 | **16** | z-fold pack | 240х152,5х4000 |  | No |  | No mark | Yes, along the rims | Chart (diagram) paper | 60 | **Laboratory equipment** Printer Epson LX 300+, etc. | 1 | 146,40 |  |
| 337 | 3717/1 | **16** | z-fold pack | 240х152,5х2000 |  | No |  | No mark | Yes, along the rims | Chart (diagram) paper | 60 | **Laboratory equipment** Printer Epson LX 300+, etc. | 1 | 73,2 |  |
| 338 | 3928 | **16** | z-fold pack | 240х305х2000 |  | No |  | No mark | Yes, along the rims | Chart (diagram) paper | 60 | **Laboratory equipment** Printer Epson LX 300+, etc. | 1 | 146,40 |  |
| 339 | 3929 | **16** | z-fold pack | 420х305х2000 |  | No |  | No mark | Yes, along the rims | Chart (diagram) paper | 60 | **Laboratory equipment** Printer Epson LX 300+, etc. | 1 | 256,20 |  |
| 340 | 10009 | **16** | z-fold pack | 210х305х2000 |  | No |  | No mark | Yes, along the rims | Chart (diagram) paper | 60 | **Laboratory equipment.**  **Geoanalyzer** «Medonik»  Printer Epson LX 300, etc. | 1 | 128,10 |  |

Design styles:

1. In the rolls with the chart paper grid, the winding of the thermal layer on the core - inward, with the photometric mark.

2. In the rolls with the chart paper grid, the winding of the thermal layer on the core - inward, without the photometric mark.

3. In the rolls with the chart paper grid, the winding of the thermal layer on the core - outward, with the photometric mark.

4. In the rolls with the chart paper grid, the winding of the thermal layer on the core - outward, without the photometric mark..

5. In the rolls without the chart paper grid, the winding of the thermal layer on the core - inward, with the photometric mark.

6. In the rolls without the chart paper grid, the winding of the thermal layer on the core - inward, without the photometric mark.

7. In the rolls without the chart paper grid, the winding of the thermal layer on the core - outward, with the photometric mark.

8. In the rolls without the chart paper grid, the winding of the thermal layer on the core - outward, without the photometric mark.

9. Z-folded with the chart paper grid.

10. Z-folded with the chart paper grid with the photometric mark.

11. Z-folded without the chart paper grid.

12. Z-folded without the chart paper grid with the photometric mark.

13. Z-folded with the chart paper grid with the photometric mark on the non-thermal layer side of paper.

14. Z-folded with the chart paper grid with two photometric marks on the paper grid.

15. Z-folded with the chart paper grid with perforation on two sides.

16. Z-folded without the chart paper grid with perforation on two sides.